{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - D E McCormick 1469"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2130-2140","2140-2150","2330-2340","2340-2350","2350-2360","2360-2370"]
[]
["NON-CLAY FRACTION"]
["Quartz",40.58507831707977,39.201715513921393,33.556317255086213,47.09715136636153,44.1790094440139,36.025770159597634]
["K-Feldspar",0.7465937132369872,0.80430947328644342,0.37302919565340215,0.38062054488629748,0.14653481045583405,0.1461527712769361]
["Plagioclase",6.4318215818754014,6.175700571871265,5.3463044328631737,6.1023273553450341,6.524703737112679,6.4866598384880971]
["Organic Carbon (TOC)",0.247,0.219,0.46600000000000003,0.50700000000000001,0.435,0.39900000000000002]
["Apatite",0,0,0,0,0,0]
["Pyrite",0,0,0.84198821358313247,0.77951072371275731,0.81616103372690163,0.91508550703108638]
["Marcasite",0,0,0,0,0,0]
["Calcite",0,0,0,0,0.23253723024326572,0.81595507434350512]
["Dolomite",0,0,0,0,0,0]
["Siderite",1.071373027090315,1.0629347544426955,0.39991825947252407,0.3937447226760582,0.49927422066808147,0.79909508451841271]
["Anatase",0.61126228647943193,0.62503249325258736,0.78462768316411668,0.69369411027739258,0.64190956970869117,0.66586073328154405]
["TOTAL",{"$f":"SUM(B9:B19)","v":49.693128925761911},{"$f":"SUM(C9:C19)","v":48.08869280677439},{"$f":"SUM(D9:D19)","v":41.768185039822562},{"$f":"SUM(E9:E19)","v":55.954048823259065},{"$f":"SUM(F9:F19)","v":53.475130045929362},{"$f":"SUM(G9:G19)","v":46.253579168537215}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",6.1263903495984469,5.5680725295742421,6.5071822049991441,5.2571430379011357,5.6973751894066496,4.8937565787451911]
["Illite+Mica",36.922501677525361,37.477010959142397,42.68524211930341,32.99720983947681,33.227260735266256,38.484655385060343]
["Chlorite",2.4580852177320973,2.6356599349753647,4.3562363986403572,2.7512255279836988,3.7012801057007723,4.9383570612857559]
["Kaolinite",4.7998938293821967,6.2305637695336333,4.6831542372345147,3.0403727713793085,3.8989539236969586,5.4296518063714974]
["TOTAL",{"$f":"SUM(B23:B26)","v":50.306871074238103},{"$f":"SUM(C23:C26)","v":51.911307193225639},{"$f":"SUM(D23:D26)","v":58.231814960177431},{"$f":"SUM(E23:E26)","v":44.045951176740957},{"$f":"SUM(F23:F26)","v":46.524869954070638},{"$f":"SUM(G23:G26)","v":53.746420831462785}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100.00000000000001},{"$f":"C27+C20","v":100.00000000000003},{"$f":"D27+D20","v":100},{"$f":"E27+E20","v":100.00000000000003},{"$f":"F27+F20","v":100},{"$f":"G27+G20","v":100}]
[]
["% Expandable Layers in I/S",16.533603884400009,18.85160461239991,14.215603156399993,14.590573862399992,14.215603156399993,14.113338418399962]
["% I/S to Illite in <1.0um Fraction",15.584468528007505,14.318453818266681,15.428294264016095,14.712691563116426,17.976825682443764,14.483402397509863]
["% Expandable I/S Layers in sample",1.0154212031865868,1.0519748427125306,0.92936604469483475,0.77095608534970694,0.81345477553080103,0.69343924993827433]
[]
[]
["Comments"]